This documentation is designed to provide guidance to customers 
on how to upgrade RSA5000/RSA3000 Spectrum Analyzers to the version in the "RSA5000(ARM)update.rar" file. 
The applicable models include RSA5065,RSA5065-TG,RSA5065N
                                                  RSA5032,RSA5032-TG,RSA5032N
                                                  RSA3015N,RSA3030,RSA3030-TG,RSA3030N
                                                  RSA3045,RSA3045-TG,RSA3045N

New versions of firmware are available at the following website:
http://int.rigol.com

[Notices]

- Please make sure that your USB disk can be read correctly. 
  RSA5000/RSA3000 is required to use an USB disk with FAT32 format. 

- During upgrade process, please do not cut off power and pull out the USB disk,
  otherwise the instrument will fail to work normally.

- During the process, the instrument cannot be in the remote mode 
  (Do not connect USB cable or the network cable).
 
- For some versions, previously saved state files cannot be used after upgrade. 
  Please make sure to keep a record of the necessary information of settings 
  before upgrade. 
 
[Upgrading Procedures]

1. Copy the upgrade file rsa5000_updatefile.bin to the root directory of the USB disk.
 
2. Insert the USB disk into the USB interface.
 
3. Find the upgrade file in the "File->File Explorer", click "File->System Update" button.

4. When the upgrading is completed, please restart your RSA5000/RSA3000.
 
[Troubleshooting]

- If you fail to upgrade, please visit the website int.rigol.com 
  to find contacts in your area. 